**Die Harderen**

**Directions for Use**

**Preparation:**

* Clean die, remove debris and visible dust.
* Shake container well to create a consistent, thin liquid. Bubbles should appear around top of liquid.
* Apply to die surface with applicator brush.
* Apply additional coats with a 10-15 second absorption time in between.
* Blot out excess liquid, do not allow pooling or puddles.
* Let set for 3-5 minutes until matte finish is visible.

**Precautions:**

* Use with adequate ventilation.
* Cap container after use.