**Top Cera Sep**

**Directions for Use**

**Preparation:**

* Clean die, removing debris and visible dust and let dry.
* Apply the first thin layer in even brush strokes over entire die margin area.
* Blow off excess liquid.
* Inspect to assure full coverage of die surface.
* Use a fine wax pencil to mark the facial margin.

**Precautions**:

* Close container immediately after each application.