**Top Die Sealer**

**Directions for use**

**Preparation:**

* Clean plaster or stone die, removing debris and visible dust.
* Using the application brush, apply the first layer in even applications over entire die margin area.
* Blow off excess liquid and allow to air dry thoroughly.
* Inspect to assure full coverage of die surface.
* Reapply die sealer for two more coats, allowing each coat to dry thoroughly before adding the next one.
* Use a fine wax pencil to mark the facial margin.

**Precautions**:

* Close container immediately after use.
* Use **Top** **Thinner** to keep viscosity fluid.